# Test of Pop semantics for Y86-64
	irmovq $0x100,%rsp  # Initialize stack pointer
	irmovq $0xABCD,%rax 
	pushq  %rax         # Put known value on stack
	popq   %rsp         # Either get 0xABCD, or 0xfc
	halt
